{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Tabelle1"],"not_rendered":{"charts":2,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":74,"n_cols":12,"rows_kept":74,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[null,"Test BBT+  -  variabler Haltepunkt (HP)",{"$nulls":9},"2016-04-06"]
[]
[null,"Anz. Fahrten","km/h","Offset","Intervall","HP (max)","HP (min)","HP (mittel)","Streu.","%","Abw.","%"]
[]
[null,"BBT 12 steps",40,2030,1955,2030,2030,2030,0,0,0,0]
[null,9,40,500,481.5270935960591,568,558,563,10,0.017761989342806393,63,0.126]
[null,8,40,1000,963.0541871921182,1050,1034,1042,16,0.015355086372360844,42,0.042]
[null,7,40,1500,1444.5812807881773,1533,1520,1526.5,13,0.008516213560432362,26.5,0.017666666666666667]
[]
[null,"BBT 12 steps",60,2030,1288,2030,2030,2030,0,0,0,0]
[null,6,60,500,317.2413793103448,595,589,592,6,0.010135135135135136,92,0.184]
[null,6,60,1000,634.4827586206897,1082,1065,1073.5,17,0.015836050302748022,73.5,0.0735]
[null,7,60,1500,951.7241379310345,1544,1530,1537,14,0.009108653220559532,37,0.024666666666666667]
[]
[null,"BBT 12 steps",90,2030,829,2030,2030,2030,0,0,0,0]
[null,8,90,500,204.1871921182266,648,620,634,28,0.04416403785488959,134,0.268]
[null,8,90,1000,408.3743842364532,1112,1090,1101,22,0.019981834695731154,101,0.101]
[null,7,90,1500,612.5615763546798,1564,1543,1553.5,21,0.013517862890247827,53.5,0.035666666666666666]
[]
[null,"BBT 10 steps",90,2030,855,2030,2030,2030,0,0,0,0]
[null,null,90,500,210.59113300492612,660,646,653,14,0.021439509954058193,153,0.306]
[null,null,90,1000,421.18226600985224,1096,1071,1083.5,25,0.023073373327180433,83.5,0.0835]
[null,null,90,1500,631.7733990147783,1573,1559,1566,14,0.008939974457215836,66,0.044]
[]
[null,"Test-Bedingungen:"]
[null,"BBT (Steps) = 12 (40, 60, 90), 10 (90)"]
[null,"Intervall (BBT) = ms, so eingelernt, dass Vmin möglichst kurz vor dem IN-Melder erreicht wird, fixiert"]
[null,"Intervall (HP) = Intervall (BBT) * HP-Offset / Blocklänge = prop. zu HP-Offset, manuell eingetragen, fixiert, IN-Ereignis erzeugen"]
[null,"Messblock = 2030 mm Blocklänge"]
[null,"HP-Offset = Distanz ab Melder von Block-Einfahrseite"]
[null,"Vmin (Loco) = 4 km/h"]
[null,"Betriebstemperatur: die kalte Lok läuft etwas langsamer, Abweichung max. +2 km/h"]
[null,"Messwerte: Verteilung nicht gewichtet"]
[null,"Messpunkt: Position Magnet (Lokmitte)"]
[]
[null,"HW/SW"]
[null,"Rocrail rev: 11058"]
[null,"Server/Viewer: Laptop i7-3612QM, 2.10 GHz, 8GB, W10 64-bit"]
[null,"Interface: CAN-GCA mit GC1e Ethernet, GC3 CS, ORD-3 Booster, GC2 I/O, TLE4905 Hall Sensoren"]
[null,"Lok: H0m, Bemo Ge 4/4 II, ESU Lokpilot micro V4.0"]
[]
[]
[null,"Offset","40 km/h","60 km/h","90 km/h"]
[null,500,563,592,634]
[null,1000,1042,1073.5,1101]
[null,1500,1526.5,1537,1553.5]
{"$rows_empty":23}
[null,null,null,"Offset genullt","40 km/h","60 km/h","90 km/h"]
[null,null,null,0,63,92,134]
[null,null,null,0,42,74,101]
[null,null,null,0,27,37,54]